# Legendary Diesel Performance Truck Pulling Rules

# Hot Street

 This is a diesel fuel only class designed for heavily modified street driven DOT legal Pickups

**Credentials**: Must be DOT legal pickup truck with valid license and registration. Vehicle must be 4x4, and ¾ or 1 ton, driver must have valid driver license. No passengers are allowed during pulling.

**Weight**: Maximum 8500 lbs with driver.

**Ballast**: Front hanging weights are allowed, hanging weight or bracket may not extend more than 60 inches from center line of front axle. No weight can be added in the cab area, all weights must be secured.

**Batteries**: Batteries must be securely mounted, and may not be mounted in driver compartment.

**Body**: Must be OEM truck body of ¾ or 1 ton, aftermarket hoods will be allowed, must have front and rear bumpers, aftermarket bumpers and rear roll pans are allowed. Must have complete running equipment installed and working. (All headlights, taillights, brake/reverse. Factory windshield and wipers)

**Brakes**: Must have 4 wheel working brakes.

**Chassis**: Must be OEM chassis of ¾ or 1 ton. Must retain all OEM chassis mounting points for front and rear suspension. Suspension lifts are allowed. Rear suspension blocking is allowed. Rear suspension air bags are allowed, but must not be inflated during pulling. Traction bars are permitted and must be weld on or bolt on type. Axles must be OEM housings optional on 1ton or smaller Trucks, OEM transmission and transfer case of 1 ton and smaller truck only. OEM style steering must be retained, additional stabilizers are allowed. Drive shaft loops & U joint shields are recommended.

**Engine**: Engine must be an OEM engine of a 1 ton or smaller truck. Head & block may have modified appearance, engine may be modified with bolt on engine modifications. May have emissions altered, and equipped with aftermarket tuning. NO DQs will be issued for smoke in any class.

**Exhaust**: All exhaust must exit rearward of cab, fender or hood stacks are allowed in this class.

**Fuel**: Fuel must be pump Fuel #1 or #2 Diesel, no race fuels allowed, and fuel tanks must be in stock location. Auxiliary fuel tanks must be securely mounted and empty of any fuel.

**Hitch**: Hitch must be receiver style hitch mounted in factory location. Hitch may have bracing in this class, braces must extend from frame down and not axle up. Bracing may not extend forward of center of rear axle, maximum hitch height must not exceed 28”, hitch must be minimum of 44” rearward of rear axle centerline to hooking point, and hooking point must have a minimum of a 3.5” diameter to hook sled.

**Injectables**: No injectables are allowed in this class, if system is installed must prove to officials that it is disabled.

**Tires**: Tires must be DOT approved tires, dual rear wheels are permitted on OEM appropriate beds only.

**Turbo**: Vehicles may have multiple turbos in this class. Aftermarket style compressor wheel and covers are allowed. Aftermarket turbos of a max size of 3.15” inlet will be allowed. **Owner will be required to make the compressor inlet accessible to officials for inspection. No turbo inlet larger than 3.15” (80mm) will be allowed in the class. All turbos will be checked!!**

**All rules are subject to officials’ final decisions, vehicles maybe entered multiple times in multiple classes if rules of classes are met. Vehicles will be allowed to enter a class up till class has started to run. All vehicles are subject to post competition inspection. Failure to abide by the rules my result in DQ. Hook fees for this class is $25.00 per hook. If multiple hooks are desired, must register for all hooks prior to start of class. You will not be able to pay for more hooks after the class begins.**